#An AiGIS data set based on Ryugu_SHAPE_SFM_49k_v20180804.
#Geophysical parameter maps are assuming a model density of 1200 kg/m^3.
## Shape model data
SHAPE = Shapemodel/SHAPE_SFM_49k_v20180804.obj
SHAPEHIGH = Shapemodel/SHAPE_SFM_3M_v20180804.obj
IMAGEMAPDIR=Images
LOOKUPDIR = ../LookUp

# Set CHANGEMODEL as FALSE to keep resolution of the displayed model as you selected.
CHANGEMODEL = FALSE
# CHANGEMODEL = TRUE

## Grid data
## GRIDR and GRIDR are mandatory.
GRIDW = Shapemodel/SHAPE_SFM_49k_v20180804_grid_white.txt
GRIDR = Shapemodel/SHAPE_SFM_49k_v20180804_grid_red.txt

## Map data
# Data in MapData and MapDataHigh will be loaded by default
#MAPDATA = RELATIVE_PATH_TO_MAPDATA_FOR_SHAPE_MODEL1
#MAPDATAHIGH = RELATIVE_PATH_TO_MAPDATA_FOR_SHAPE_MODEL2

## Graph map data
#CHARTDATA= RELATIVE_PATH_TO_PLOT_DATA

## Mandatory directories.
# MapData
# MapDataHigh
# Shapemodel